{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["100 ADS","Conversions","Options","Gas Tables"],"not_rendered":{"macros":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"100 ADS","index":0,"n_rows":245,"n_cols":12,"rows_kept":245,"merged":[[1,0,7,0],[1,2,1,5],[2,2,2,5],[3,2,3,5],[4,2,4,5],[6,2,6,5],[7,2,7,5],[8,2,8,5],[9,2,9,5],[10,2,10,5],[11,2,11,5],[12,2,12,5],[13,2,13,5],[14,2,14,5],[15,2,15,5],[16,0,17,0],[16,2,16,5],[17,2,17,5],[27,1,30,5]],"flags":["formulas_cached_only"]}
["Compod® Application Data Sheet (May require one for each unit in the order)",{"$nulls":6},"1 (default)","19.2K (default)","Even (default)","34-12 (default)","4 ms (default)"]
["For Sierra Use Only","Sales Order Number",{"$nulls":5},2,"9.6K","Odd","43-21","8 ms "]
[null,"Line Item Number",{"$nulls":5},3,"38.4K","None","21-43","12 ms"]
[null,"Serial Number",{"$nulls":5},4,"57.6K",null,"12-34","16 ms"]
[null,"Sierra Representative",{"$nulls":5},5,{"$nulls":3},"20 ms"]
[null,"AE Order Approval/Date",{"$nulls":5},6,{"$nulls":3},"24 ms"]
[null,"Checked/Date",{"$nulls":5},7,{"$nulls":3},"28 ms"]
[null,null,"Enter Information Below",{"$nulls":4},8,{"$nulls":3},"32 ms"]
[null,"Purchase Order Number",{"$nulls":5},9,{"$nulls":3},"36 ms"]
[null,"Distributor/Representative Company",{"$nulls":5},10,{"$nulls":3},"40 ms"]
["Distributor Information","Distributor Contact Name",{"$nulls":5},11,{"$nulls":3},"44 ms"]
[null,"Distributor Telephone + Fax Number",{"$nulls":5},12,{"$nulls":3},"48 ms"]
[null,"Distributor E-mail address",{"$nulls":5},13,{"$nulls":3},"52 ms"]
[null,"Customer Purchase Order Number",{"$nulls":5},14,{"$nulls":3},"56 ms"]
[null,"Customer Company Name                      (will be noted on the Calibration Certificate)",{"$nulls":5},15,{"$nulls":3},"60 ms"]
["End user Information","Customer location (City + Country)",{"$nulls":5},16,{"$nulls":3},"64 ms"]
[null,"Technical Contact Name",{"$nulls":5},17,{"$nulls":3},"68 ms"]
[null,"Contact Phone # and E-mail address",{"$nulls":5},18,{"$nulls":3},"72 ms"]
[null,"Model Number",{"$nulls":5},19,{"$nulls":3},"76 ms"]
["Com Information","Network ID#",{"$nulls":5},20,{"$nulls":3},"80 ms"]
[null,"Baud Rate",null,null," ",null,null,21,{"$nulls":3},"84 ms"]
[null,"Parity",{"$nulls":5},22,{"$nulls":3},"88 ms"]
[null,"Tx Delay",{"$nulls":5},23,{"$nulls":3},"92 ms"]
[null,"Tag Info (8 charactors max.)",{"$nulls":5},24,{"$nulls":3},"96 ms"]
[null,"Modbus Byte order",{"$nulls":5},25,{"$nulls":3},"100 ms"]
["Pulse Output","Pulse Width (2.5 to 500 ms)",{"$nulls":5},26,{"$nulls":3},"104 ms"]
[null,"Units Per pulse (0 to 255)",{"$nulls":5},27,{"$nulls":3},"108 ms"]
["Special Instructions",{"$nulls":6},28,{"$nulls":3},"112 ms"]
[{"$nulls":7},29,{"$nulls":3},"116 ms"]
[{"$nulls":7},30,{"$nulls":3},"120 ms"]
[{"$nulls":7},31,{"$nulls":3},"124 ms"]
[{"$nulls":7},32,{"$nulls":3},"128 ms"]
[{"$nulls":7},33,{"$nulls":3},"132 ms"]
[{"$nulls":7},34,{"$nulls":3},"136 ms"]
[{"$nulls":7},35,{"$nulls":3},"140 ms"]
[{"$nulls":7},36,{"$nulls":3},"144 ms"]
[{"$nulls":7},37,{"$nulls":3},"148 ms"]
[{"$nulls":7},38,{"$nulls":3},"152 ms"]
[{"$nulls":7},39,{"$nulls":3},"156 ms"]
[{"$nulls":7},40,{"$nulls":3},"160 ms"]
[{"$nulls":7},41,{"$nulls":3},"164 ms"]
[{"$nulls":7},42,{"$nulls":3},"168 ms"]
[{"$nulls":7},43,{"$nulls":3},"172 ms"]
[{"$nulls":7},44,{"$nulls":3},"176 ms"]
[{"$nulls":7},45,{"$nulls":3},"180 ms"]
[{"$nulls":7},46,{"$nulls":3},"184 ms"]
[{"$nulls":7},47,{"$nulls":3},"188 ms"]
[{"$nulls":7},48,{"$nulls":3},"192 ms"]
[{"$nulls":7},49,{"$nulls":3},"196 ms"]
[{"$nulls":7},52,{"$nulls":3},"208 ms"]
[{"$nulls":7},53,{"$nulls":3},"212 ms"]
[{"$nulls":7},54,{"$nulls":3},"216 ms"]
[{"$nulls":7},55,{"$nulls":3},"220 ms"]
[{"$nulls":7},56,{"$nulls":3},"224 ms"]
[{"$nulls":7},57,{"$nulls":3},"228 ms"]
[{"$nulls":7},58,{"$nulls":3},"232 ms"]
[{"$nulls":7},59,{"$nulls":3},"236 ms"]
[{"$nulls":7},60,{"$nulls":3},"240 ms"]
[{"$nulls":7},61,{"$nulls":3},"244 ms"]
[{"$nulls":7},62,{"$nulls":3},"248 ms"]
[{"$nulls":7},63,{"$nulls":3},"252 ms"]
[{"$nulls":7},64]
[{"$nulls":7},65]
[{"$nulls":7},66]
[{"$nulls":7},67]
[{"$nulls":7},68]
[{"$nulls":7},69]
[{"$nulls":7},70]
[{"$nulls":7},71]
[{"$nulls":7},72]
[{"$nulls":7},73]
[{"$nulls":7},74]
[{"$nulls":7},75]
[{"$nulls":7},76]
[{"$nulls":7},77]
[{"$nulls":7},78]
[{"$nulls":7},79]
[{"$nulls":7},80]
[{"$nulls":7},81]
[{"$nulls":7},82]
[{"$nulls":7},83]
[{"$nulls":7},84]
[{"$nulls":7},85]
[{"$nulls":7},86]
[{"$nulls":7},87]
[{"$nulls":7},88]
[{"$nulls":7},89]
[{"$nulls":7},90]
[{"$nulls":7},91]
[{"$nulls":7},92]
[{"$nulls":7},93]
[{"$nulls":7},94]
[{"$nulls":7},95]
[{"$nulls":7},96]
[{"$nulls":7},97]
[{"$nulls":7},98]
[{"$nulls":7},99]
[{"$nulls":7},100]
[{"$nulls":7},101]
[{"$nulls":7},102]
[{"$nulls":7},103]
[{"$nulls":7},104]
[{"$nulls":7},105]
[{"$nulls":7},106]
[{"$nulls":7},107]
[{"$nulls":7},108]
[{"$nulls":7},109]
[{"$nulls":7},110]
[{"$nulls":7},111]
[{"$nulls":7},112]
[{"$nulls":7},113]
[{"$nulls":7},114]
[{"$nulls":7},115]
[{"$nulls":7},116]
[{"$nulls":7},117]
[{"$nulls":7},118]
[{"$nulls":7},119]
[{"$nulls":7},120]
[{"$nulls":7},121]
[{"$nulls":7},122]
[{"$nulls":7},123]
[{"$nulls":7},124]
[{"$nulls":7},125]
[{"$nulls":7},126]
[{"$nulls":7},127]
[{"$nulls":7},128]
[{"$nulls":7},129]
[{"$nulls":7},130]
[{"$nulls":7},131]
[{"$nulls":7},132]
[{"$nulls":7},133]
[{"$nulls":7},134]
[{"$nulls":7},135]
[{"$nulls":7},136]
[{"$nulls":7},137]
[{"$nulls":7},138]
[{"$nulls":7},139]
[{"$nulls":7},140]
[{"$nulls":7},141]
[{"$nulls":7},142]
[{"$nulls":7},143]
[{"$nulls":7},144]
[{"$nulls":7},145]
[{"$nulls":7},146]
[{"$nulls":7},147]
[{"$nulls":7},148]
[{"$nulls":7},149]
[{"$nulls":7},150]
[{"$nulls":7},151]
[{"$nulls":7},152]
[{"$nulls":7},153]
[{"$nulls":7},154]
[{"$nulls":7},155]
[{"$nulls":7},156]
[{"$nulls":7},157]
[{"$nulls":7},158]
[{"$nulls":7},159]
[{"$nulls":7},160]
[{"$nulls":7},161]
[{"$nulls":7},162]
[{"$nulls":7},163]
[{"$nulls":7},164]
[{"$nulls":7},165]
[{"$nulls":7},166]
[{"$nulls":7},167]
[{"$nulls":7},168]
[{"$nulls":7},169]
[{"$nulls":7},170]
[{"$nulls":7},171]
[{"$nulls":7},172]
[{"$nulls":7},173]
[{"$nulls":7},174]
[{"$nulls":7},175]
[{"$nulls":7},176]
[{"$nulls":7},177]
[{"$nulls":7},178]
[{"$nulls":7},179]
[{"$nulls":7},180]
[{"$nulls":7},181]
[{"$nulls":7},182]
[{"$nulls":7},183]
[{"$nulls":7},184]
[{"$nulls":7},185]
[{"$nulls":7},186]
[{"$nulls":7},187]
[{"$nulls":7},188]
[{"$nulls":7},189]
[{"$nulls":7},190]
[{"$nulls":7},191]
[{"$nulls":7},192]
[{"$nulls":7},193]
[{"$nulls":7},194]
[{"$nulls":7},195]
[{"$nulls":7},196]
[{"$nulls":7},197]
[{"$nulls":7},198]
[{"$nulls":7},199]
[{"$nulls":7},200]
[{"$nulls":7},201]
[{"$nulls":7},202]
[{"$nulls":7},203]
[{"$nulls":7},204]
[{"$nulls":7},205]
[{"$nulls":7},206]
[{"$nulls":7},207]
[{"$nulls":7},208]
[{"$nulls":7},209]
[{"$nulls":7},210]
[{"$nulls":7},211]
[{"$nulls":7},212]
[{"$nulls":7},213]
[{"$nulls":7},214]
[{"$nulls":7},215]
[{"$nulls":7},216]
[{"$nulls":7},217]
[{"$nulls":7},218]
[{"$nulls":7},219]
[{"$nulls":7},220]
[{"$nulls":7},221]
[{"$nulls":7},222]
[{"$nulls":7},223]
[{"$nulls":7},224]
[{"$nulls":7},225]
[{"$nulls":7},226]
[{"$nulls":7},227]
[{"$nulls":7},228]
[{"$nulls":7},229]
[{"$nulls":7},230]
[{"$nulls":7},231]
[{"$nulls":7},232]
[{"$nulls":7},233]
[{"$nulls":7},234]
[{"$nulls":7},235]
[{"$nulls":7},236]
[{"$nulls":7},237]
[{"$nulls":7},238]
[{"$nulls":7},239]
[{"$nulls":7},240]
[{"$nulls":7},241]
[{"$nulls":7},242]
[{"$nulls":7},243]
[{"$nulls":7},244]
[{"$nulls":7},245]
[{"$nulls":7},246]
[{"$nulls":7},247]

{"sheet":"Conversions","index":1,"n_rows":47,"n_cols":17,"rows_kept":47,"hidden":true,"flags":["formulas_cached_only"]}
[{"$nulls":13},1,"Steel weldless new",0.1,"mm"]
[null,"Meter",1,1,{"$nulls":9},2,"Steel weldless used",0.2,"mm"]
[null,"cm",0.01,2,{"$nulls":9},3,"Steel weldless corroded",0.4,"mm"]
[null,"mm",0.001,3,{"$nulls":9},4,"Steel weldless very corroded",2,"mm"]
[null,"Inch",0.0254,4,{"$nulls":9},5,"Steel welded new",0.1,"mm"]
[null,"Feet",0.3048,5,{"$nulls":9},6,"Steel welded old",0.3,"mm"]
[{"$nulls":13},7,"Steel welded corroded",1,"mm"]
[null,"Conversion table is to get the actual flow to NLPM.Multiply the actual flow by the mentioned factor to get NLPM, Note that the density is a variable in this table.",{"$nulls":11},8,"Steel welded very corroded",3,"mm"]
[null,"Selected gas :",{"$error":"#REF!"},"Density",{"$error":"#REF!"},"Gr/L @ 0C",{"$nulls":7},9,"Brass/glass/lead/copper",0.001,"mm"]
[null,"Conversion factors",null,"Ref temp.",{"$nulls":9},10,"Galvanised pipe",0.15,"mm"]
[1,"Gr/hr",{"$error":"#REF!"},null,1,{"$nulls":8},11,"Rivetted steel pipe",0.9,"mm"]
[2,"Gr/min",{"$error":"#REF!"},null,2,{"$nulls":8},12,"Cast iron pipe",1,"mm"]
[3,"Gr/sec",{"$error":"#REF!"},null,3,{"$nulls":8},13,"Concrete pipe new",0.8,"mm"]
[4,"Kg/hr",{"$error":"#REF!"},null,4,{"$nulls":8},14,"Concrete pipe rough",3,"mm"]
[5,"Kg/min",{"$error":"#REF!"},null,5,{"$nulls":8},15,"Masonry (Brick)",1.3,"mm"]
[6,"Kg/sec",{"$error":"#REF!"},null,6]
[7,"Lbs/hr",{"$error":"#REF!"},null,7]
[8,"Lbs/min",{"$error":"#REF!"},null,8]
[9,"Lbs/sec",{"$error":"#REF!"},null,9]
[10,"NLPM",1,0,10]
[11,"NLPH",0.016666666666666666,0,11]
[12,"NM3/hr",16.666666666666668,0,12]
[13,"NM3/min",1000,0,13]
[14,"NML/min",0.001,0,14]
[15,"SCCM",0.0009283018629718768,21.1,15]
[16,"SCFM",26.28950875936355,21.1,16]
[17,"SCFH",0.43815847932272584,21.1,17]
[18,"SLPH",0.015471697716197946,21.1,18]
[19,"SLPM",0.9283018629718768,21.1,19]
[]
[null,"Atm",0.987,1]
[null,"Bar",1,2]
[null,"cm H2O",101.9744,3]
[null,"ft. H2O",33.47,4]
[null,"in. H2O",401.6,5]
[null,"in. Hg",29.53,6]
[null,"Kg/cm2",1.02,7]
[null,"kPa",100,8]
[null,"mBar",1000,9]
[null,"mm H2O",1019.7443,10]
[null,"mmHg",750,11]
[null,"Pa",100000,12]
[null,"Psi",14.50377,13]
[]
[null,"Celsius",20,20,1]
[null,"Fahrenheit",-6.666666666666667,68,2]
[null,"Kelvin",-253.15,293.15,3]

{"sheet":"Options","index":2,"n_rows":29,"n_cols":5,"rows_kept":29,"hidden":true,"flags":["formulas_cached_only"]}
[]
["This page is there because the coversion factors from and to Mass change if the gas changes. This is required when one converts a flow for a 800 series to a different gas (=different density)"]
["The different density of the gas selected under Conversions on the selection page is shown in C6 of this page."]
[]
[]
[]
[]
["Conversion table is from NLPM and than divide by the mentioned factor, Note that the density is a variable in this table."]
["Selected gas :",{"$error":"#REF!"},"Density",{"$error":"#REF!"},"Gr/L @ 0C"]
["Conversion factors",null,"Ref temp."]
[1,"Gr/hr",{"$error":"#REF!"},null,1]
[2,"Gr/min",{"$error":"#REF!"},null,2]
[3,"Gr/sec",{"$error":"#REF!"},null,3]
[4,"Kg/hr",{"$error":"#REF!"},null,4]
[5,"Kg/min",{"$error":"#REF!"},null,5]
[6,"Kg/sec",{"$error":"#REF!"},null,6]
[7,"Lbs/hr",{"$error":"#REF!"},null,7]
[8,"Lbs/min",{"$error":"#REF!"},null,8]
[9,"Lbs/sec",{"$error":"#REF!"},null,9]
[10,"NLPM",1,0,10]
[11,"NLPH",0.016666666666666666,0,11]
[12,"NM3/hr",16.666666666666668,0,12]
[13,"NM3/min",1000,0,13]
[14,"NML/min",0.001,0,14]
[15,"SCCM",0.0009283018629718768,21.1,15]
[16,"SCFM",26.28950875936355,21.1,16]
[17,"SCFH",0.43815847932272584,21.1,17]
[18,"SLPH",0.015471697716197946,21.1,18]
[19,"SLPM",0.9283018629718768,21.1,19]

{"sheet":"Gas Tables","index":3,"n_rows":141,"n_cols":22,"rows_kept":141,"hidden":true,"flags":["formulas_cached_only"]}
[null,"Gas name","Formula","Cal gas","Formula","K-fact ref gas","K-Fact N2","Cp [Cal/gr]","Density @ 0","Mol. Weight","Critical Temp","Dyn. Visc.","Spec. Heat","Heat Cond","Remarks","Mat. Oring","Mat. Valve seat","Remarks","Max. 600","HV Speed","Ignition temp."]
[{"$nulls":7},"Cal/gr","Kg/M3",null,"Degrees K","Pa.s at 25 C","kJ/Kg K","W/m K","Heat Cond",{"$nulls":3},"NMPS","NMPS","Degr. C"]
[{"$nulls":11},"=Ns/M2","Cp","Labda","n"]
[null,"Same gas",{"$nulls":3},1,1,1,2,1,{"$nulls":11},3]
[1,"Acetylene","C2H2","Ethylene","C2H4",{"v":0.973,"d":"0.9730"},{"v":0.58,"d":"0.5800"},0.4036,1.1715,{"v":0.88,"d":"0.8800"},308.33,1.046e-05,{"v":1.687,"d":"1.6870"},0.0215,null,"Viton","Viton","Flammable, Explosive acetylide is formed in contact with Copper, Silver, Mercury.",0,null,305,4]
[2,"Air","Air","Air","Air",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},{"v":0.24,"d":"0.2400"},{"v":1.293,"d":"1.2930"},{"v":1,"d":"1.0000"},132.42,1.83e-05,{"v":1.004,"d":"1.0040"},0.026,null,"Viton","Viton","None",94,132,null,5]
[3,"Allene(Propadiene)","C3H4","Freon 14","CF4",{"v":0.934,"d":"0.9340"},{"v":0.43,"d":"0.4300"},{"v":0.352,"d":"0.3520"},{"v":1.787,"d":"1.7870"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",null,0,null,null,6]
[4,"Ammonia","NH3","Nitrogen probably","N2O/N2",{"v":1.028,"d":"1.0280"},{"v":0.73,"d":"0.7300"},{"v":0.492,"d":"0.4920"},{"v":0.76,"d":"0.7600"},{"v":0.941,"d":"0.9410"},{"v":405.5,"d":"405.5000"},1.002e-05,{"v":2.086,"d":"2.0860"},0.0216,"At 0 C only","Neoprene","Kalrez","Poison, very flammable",88,null,630,7]
[5,"Argon","Ar","Argon","Ar",{"v":1,"d":"1.0000"},{"v":1.45,"d":"1.4500"},0.1244,{"v":1.782,"d":"1.7820"},{"v":1.04,"d":"1.0400"},{"v":150.86,"d":"150.8600"},2.28e-05,0.5216,0.01782,null,"Viton","Viton","Heavier than Air",132,null,null,8]
[6,"Arsine","AsH3","Nitrogen probably","N2O/N2",{"v":0.943,"d":"0.9430"},{"v":0.67,"d":"0.6700"},0.1167,{"v":3.478,"d":"3.4780"},{"v":0.88,"d":"0.8800"},{"v":373,"d":"373.0000"},1.604e-05,{"v":0.494,"d":"0.4940"},null,null,"Viton","Kalrez","Strong poison, flammable, heavier than air",0,null,null,9]
[7,"Boron Trichloride","BCL3","Freon 14","CF4",{"v":0.891,"d":"0.8910"},{"v":0.41,"d":"0.4100"},0.1279,{"v":5.227,"d":"5.2270"},{"v":0.88,"d":"0.8800"},{"v":452,"d":"452.0000"},null,0.5344,0.011,"below 1 bar","Viton","Kalrez","Poison, corrosive, heavier than air",{"$nulls":3},10]
[8,"Boron Trifluoride","BF3","Freon 14","CF4",{"v":1.108,"d":"1.1080"},{"v":0.51,"d":"0.5100"},0.1778,{"v":3.025,"d":"3.0250"},{"v":0.88,"d":"0.8800"},{"v":260.8,"d":"260.8000"},1.7e-05,0.7452,0.01911,"below 1 bar","Viton","Kalrez","Poison, corrosive, heavier than air",{"$nulls":3},11]
[9,"Bromine","Br2","Nitrogen probably","N2O/N2",{"v":1.14,"d":"1.1400"},{"v":0.81,"d":"0.8100"},0.0539,{"v":7.13,"d":"7.1300"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton",{"$nulls":4},12]
[10,"Boron Tribromide ","BBr3","Freon 14","CF4",{"v":0.826,"d":"0.8260"},{"v":0.38,"d":"0.3800"},0.0647,{"v":11.18,"d":"11.1800"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},13]
[11,"Bromine Pentafluoride","BrF5","Freon 14","CF4",{"v":0.565,"d":"0.5650"},{"v":0.26,"d":"0.2600"},0.1369,{"v":7.803,"d":"7.8030"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},14]
[12,"Bromine Trifluoride","BrF3","Freon 14","CF4",{"v":0.826,"d":"0.8260"},{"v":0.38,"d":"0.3800"},0.1161,{"v":6.108,"d":"6.1080"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},15]
[13,"Bromotrifluoromethane (Freon 13 B1)","CBrF3","Freon 14","CF4",{"v":0.804,"d":"0.8040"},{"v":0.37,"d":"0.3700"},0.1113,{"v":6.644,"d":"6.6440"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},16]
[14,"1,3 Butadiene","C4H6","Freon 14","CF4",{"v":0.695,"d":"0.6950"},{"v":0.32,"d":"0.3200"},0.3514,{"v":2.413,"d":"2.4130"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Flammable, Polymerisates easily, light narcotic",null,null,415,17]
[15,"Butane","C4H10","Freon 14","CF4",{"v":0.565,"d":"0.5650"},{"v":0.26,"d":"0.2600"},0.4007,{"v":2.593,"d":"2.5930"},{"v":0.88,"d":"0.8800"},{"v":425.16,"d":"425.1600"},7.51e-06,{"v":1.734,"d":"1.7340"},0.01623,null,"Viton","Viton","Flammable, heavier than air,is narcotic",null,null,365,18]
[16,"1 Butane","C4H8","Freon 14","CF4",{"v":0.652,"d":"0.6520"},{"v":0.3,"d":"0.3000"},0.3648,{"v":2.503,"d":"2.5030"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Flammable, heavier then air, explosive mixture with air, light narcotic",null,null,440,19]
[17,"2 Butane","C4H8 CIS","Freon 14","CF4",{"v":0.704,"d":"0.7040"},{"v":0.324,"d":"0.3240"},{"v":0.336,"d":"0.3360"},{"v":2.503,"d":"2.5030"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Flammable, heavier then air, explosive mixture with air, light narcotic",{"$nulls":3},20]
[18,"2 Butane","C4H8 TRANS","Freon 14","CF4",{"v":0.632,"d":"0.6320"},{"v":0.291,"d":"0.2910"},{"v":0.374,"d":"0.3740"},{"v":2.503,"d":"2.5030"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Flammable, heavier then air, explosive mixture with air, light narcotic",{"$nulls":3},21]
[19,"Carbon Dioxide","CO2","Nitrogen probably","N2O/N2",{"v":1.042,"d":"1.0420"},{"v":0.741,"d":"0.7410"},0.2016,{"v":1.964,"d":"1.9640"},{"v":0.941,"d":"0.9410"},{"v":304.21,"d":"304.2100"},1.4833e-05,{"v":0.85,"d":"0.8500"},0.0164,null,"Viton","Viton",null,98,null,null,22]
[20,"Carbon Disulfide","CS2","Ethylene","C2H4",{"v":1.007,"d":"1.0070"},{"v":0.6,"d":"0.6000"},0.1428,{"v":3.397,"d":"3.3970"},{"v":0.941,"d":"0.9410"},{"$nulls":5},"Viton","Viton",{"$nulls":4},23]
[21,"Carbon Monoxide","CO","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.2488,{"v":1.25,"d":"1.2500"},{"v":1,"d":"1.0000"},null,1.77e-05,{"v":1.042,"d":"1.0420"},0.0249,null,"Viton","Viton",null,96,null,null,24]
[22,"Carbon Tetrachloride","CCL4","Freon 14","CF4",{"v":0.673,"d":"0.6730"},{"v":0.31,"d":"0.3100"},0.1655,{"v":6.86,"d":"6.8600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},25]
[23,"Carbon Tetrafluoride","CF4","Freon 14","CF4",{"v":0.913,"d":"0.9130"},{"v":0.42,"d":"0.4200"},0.1654,{"v":3.926,"d":"3.9260"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},26]
[24,"Carbonyl Fluoride","COF2","Ethylene","C2H4",{"v":0.907,"d":"0.9070"},{"v":0.54,"d":"0.5400"},{"v":0.171,"d":"0.1710"},{"v":2.945,"d":"2.9450"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Poison, corrosive, heavier than air, hydroscopic",{"$nulls":3},27]
[25,"Carbonyl Sulfide","COS","Nitrogen probably","N2O/N2",{"v":0.929,"d":"0.9290"},{"v":0.66,"d":"0.6600"},0.1651,{"v":2.68,"d":"2.6800"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton","Poison, flammable, explosive if mixed with air.",{"$nulls":3},28]
[26,"Chlorine","CL2","Nitrogen","N2",{"v":0.86,"d":"0.8600"},{"v":0.86,"d":"0.8600"},0.1144,{"v":3.163,"d":"3.1630"},{"v":1,"d":"1.0000"},null,1.355e-05,{"v":0.485,"d":"0.4850"},0.00884,"below 1 bar","Viton","Kalrez","Poison, Corrosive, bijtend on skin, passiveren,  clean metel required use graphite and silicone.",81,null,null,29]
[27,"Chlorine Trifluoride","CLF3","Freon 14","CF4",{"v":0.869,"d":"0.8690"},{"v":0.4,"d":"0.4000"},{"v":0.165,"d":"0.1650"},{"v":4.125,"d":"4.1250"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},30]
[28,"Chlorodifluoromethane (Freon 22)","CHCLF2","Freon 14","CF4",{"v":1,"d":"1.0000"},{"v":0.46,"d":"0.4600"},0.1544,{"v":3.858,"d":"3.8580"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},31]
[29,"Chloroform","CHCL3","Freon 14","CF4",{"v":0.847,"d":"0.8470"},{"v":0.39,"d":"0.3900"},0.1309,{"v":5.326,"d":"5.3260"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},32]
[30,"Chloropentafluoroethane (Freon 115)","C2CLF5","Freon 14","CF4",{"v":0.521,"d":"0.5210"},{"v":0.24,"d":"0.2400"},{"v":0.164,"d":"0.1640"},{"v":6.892,"d":"6.8920"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},33]
[31,"Chlorotrifluoromethane (Freon 13)","CCLF3","Freon 14","CF4",{"v":0.826,"d":"0.8260"},{"v":0.38,"d":"0.3800"},{"v":0.153,"d":"0.1530"},{"v":4.66,"d":"4.6600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Thermal and chemical very stable, heavier than air",{"$nulls":3},34]
[32,"Cyanogen","C2N2","Ethylene","C2H4",0.7526,{"v":0.61,"d":"0.6100"},0.2613,{"v":2.322,"d":"2.3220"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},35]
[33,"Cyanogen Chloride","CLCN","Ethylene","C2H4",{"v":1.024,"d":"1.0240"},{"v":0.61,"d":"0.6100"},0.1739,{"v":2.742,"d":"2.7420"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Kalrez","Poison, corrosive, bijtend, heavier than air ",{"$nulls":3},36]
[34,"Cyclopropane","C3H5","Freon 14","CF4",{"v":1,"d":"1.0000"},{"v":0.46,"d":"0.4600"},0.3177,{"v":1.877,"d":"1.8770"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},37]
[35,"Deuterium","D2","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},{"v":1.722,"d":"1.7220"},{"v":1.799,"d":"1.7990"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton","Flammable, much lighter than air, explosive with air, at high outflow self-ignition danger, heavy Hydrogen",{"$nulls":3},38]
[36,"Diborane","B2H6","Freon 14","CF4",{"v":0.956,"d":"0.9560"},{"v":0.508,"d":"0.5080"},{"v":0.508,"d":"0.5080"},{"v":1.235,"d":"1.2350"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Very poisonous, self-igniting, lighter than air, chemical and thermal unstable,mostly diluted",{"$nulls":3},39]
[37,"Dibromodifluoromethane","CBr2F2","Freon 14","CF4",{"v":0.413,"d":"0.4130"},{"v":0.19,"d":"0.1900"},{"v":0.15,"d":"0.1500"},{"v":9.362,"d":"9.3620"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},40]
[38,"Dibromethane","CH2Br2","Freon 14","CF4",{"v":1.021,"d":"1.0210"},{"v":0.47,"d":"0.4700"},{"v":0.075,"d":"0.0750"},{"v":7.76,"d":"7.7600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},41]
[39,"Dichlorodifluoromethane (Freon 12)","CCL2F2","Freon 14","CF4",{"v":0.76,"d":"0.7600"},{"v":0.35,"d":"0.3500"},0.1432,{"v":5.395,"d":"5.3950"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","heavier than air, narcotic, chemical and thermal stable",{"$nulls":3},42]
[40,"Dichlorofluoromethane (Freon 21)","CHCL2F","Freon 14","CF4",{"v":0.913,"d":"0.9130"},{"v":0.42,"d":"0.4200"},{"v":0.14,"d":"0.1400"},{"v":4.592,"d":"4.5920"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Poison, heavier than air, slow reaction",{"$nulls":3},43]
[41,"Dichloromethylsilane","(CH3)2SiCL2","Freon 14","CF4",{"v":0.543,"d":"0.5430"},{"v":0.25,"d":"0.2500"},0.1882,{"v":5.758,"d":"5.7580"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},44]
[42,"Dichlorosilane","SiH2CL2","Freon 14","CF4",{"v":0.869,"d":"0.8690"},{"v":0.4,"d":"0.4000"},{"v":0.15,"d":"0.1500"},{"v":4.506,"d":"4.5060"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Poison, flammable, corrosive, bijtend, heavier than air",{"$nulls":3},45]
[43,"1,2 Dichlorotetrafluoroethane (Freon 14)","C2CL2F4","Freon 14","CF4",{"v":0.478,"d":"0.4780"},{"v":0.22,"d":"0.2200"},{"v":0.16,"d":"0.1600"},{"v":7.626,"d":"7.6260"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},46]
[44,"1,1 Difluoroethylene (Freon 1132A)","C2H2F2","Freon 14","CF4",{"v":0.934,"d":"0.9340"},{"v":0.43,"d":"0.4300"},{"v":0.224,"d":"0.2240"},{"v":2.857,"d":"2.8570"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},47]
[45,"Digester Gas","?","Digester Gas","?",{"$nulls":13},81,null,null,48]
[46,"Dimethylamine","(CH3)2NH","Freon 14","CF4",{"v":0.804,"d":"0.8040"},{"v":0.37,"d":"0.3700"},{"v":0.366,"d":"0.3660"},{"v":2.011,"d":"2.0110"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},49]
[47,"Dimethyl Ether","(CH3)2O","Freon 14","CF4",{"v":0.847,"d":"0.8470"},{"v":0.39,"d":"0.3900"},0.3414,{"v":2.055,"d":"2.0550"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},50]
[48,"2,2 Dimethylpropane","C3H12","Freon 14","CF4",{"v":0.423,"d":"0.4230"},{"v":0.22,"d":"0.2200"},0.3914,{"v":3.219,"d":"3.2190"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},51]
[49,"Ethane","C2H6","Freon 14","CF4",{"v":1.083,"d":"1.0830"},{"v":0.5,"d":"0.5000"},0.4097,{"v":1.342,"d":"1.3420"},{"v":0.88,"d":"0.8800"},{"v":305.33,"d":"305.3300"},9.43e-06,{"v":1.757,"d":"1.7570"},0.0212,null,"Viton","Viton",null,73,null,null,52]
[50,"Ethanol","C2H6O","Freon 14","CF4",{"v":0.856,"d":"0.8560"},{"v":0.39,"d":"0.3900"},0.3395,{"v":2.055,"d":"2.0550"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},53]
[51,"Ethyl Acetylene","C4H6","Freon 14","CF4",{"v":0.703,"d":"0.7030"},{"v":0.32,"d":"0.3200"},0.3513,{"v":2.413,"d":"2.4130"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Flammable, heavier than air, is narcotic, explosive with Copper, Silver and mercury",{"$nulls":3},54]
[52,"Ethyl Chloride","C2H5CL","Freon 14","CF4",{"v":0.84,"d":"0.8400"},{"v":0.39,"d":"0.3900"},{"v":0.244,"d":"0.2440"},{"v":2.879,"d":"2.8790"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Flammable, Poison, heavier than air, strongly narcotic, ",{"$nulls":3},55]
[53,"Ethylene","C2H4","Ethylene","C2H4",{"v":1,"d":"1.0000"},{"v":0.6,"d":"0.6000"},{"v":0.365,"d":"0.3650"},{"v":1.251,"d":"1.2510"},{"v":0.88,"d":"0.8800"},{"v":282.343,"d":"282.3430"},1.04e-05,{"v":1.538,"d":"1.5380"},0.0208,null,"Viton","Viton",null,57,null,null,56]
[54,"Ethylene Oxide","C2H4O ","Freon 14","CF4",{"v":1.13,"d":"1.1300"},{"v":0.52,"d":"0.5200"},{"v":0.268,"d":"0.2680"},{"v":1.965,"d":"1.9650"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},57]
[55,"Fluorine","F2","Nitrogen","N2",{"v":0.98,"d":"0.9800"},{"v":0.98,"d":"0.9800"},0.1873,{"v":1.695,"d":"1.6950"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},58]
[56,"Fluoroform (Freon 23)","CHF3","Freon 14","CF4",{"v":1.086,"d":"1.0860"},{"v":0.5,"d":"0.5000"},{"v":0.176,"d":"0.1760"},{"v":3.127,"d":"3.1270"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},59]
[57,"Freon 11","CCL3F","Freon 14","CF4",{"v":0.717,"d":"0.7170"},{"v":0.33,"d":"0.3300"},0.1357,{"v":6.129,"d":"6.1290"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},60]
[58,"Freon 12","CCL2F2","Freon 14","CF4",{"v":0.76,"d":"0.7600"},{"v":0.35,"d":"0.3500"},0.1432,{"v":5.395,"d":"5.3950"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","heavier than air, narcotic, chemical and thermal stable",33,null,null,61]
[59,"Freon 13","CCLF3","Freon 14","CF4",{"v":0.826,"d":"0.8260"},{"v":0.38,"d":"0.3800"},{"v":0.153,"d":"0.1530"},{"v":4.66,"d":"4.6600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Thermal and chemical very stable, heavier than air",{"$nulls":3},62]
[60,"Freon 13 B1","CBrF3","Freon 14","CF4",{"v":0.804,"d":"0.8040"},{"v":0.37,"d":"0.3700"},0.1113,{"v":6.644,"d":"6.6440"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","used as fire extinguisher gas",{"$nulls":3},63]
[61,"Freon 14","CF4","Freon 14","CF4",{"v":1,"d":"1.0000"},{"v":0.42,"d":"0.4200"},0.1654,{"v":3.926,"d":"3.9260"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},64]
[62,"Freon 21","CHCL2F","Freon 14","CF4",{"v":0.913,"d":"0.9130"},{"v":0.42,"d":"0.4200"},{"v":0.14,"d":"0.1400"},{"v":4.592,"d":"4.5920"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Poison, heavier than air,slow reaction",{"$nulls":3},65]
[63,"Freon 22","CHCLF2","Freon 14","CF4",{"v":1.095,"d":"1.0950"},{"v":0.26,"d":"0.2600"},0.1544,{"v":3.858,"d":"3.8580"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Narcotic, heavier than air, not flammable, chemical and thermal stable",{"$nulls":3},66]
[64,"Freon 113","CCL2FCCLF2","Freon 14","CF4",{"v":0.434,"d":"0.4340"},{"v":0.2,"d":"0.2000"},{"v":0.161,"d":"0.1610"},{"v":8.36,"d":"8.3600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},67]
[65,"Freon 114","C2CL2F4","Freon 14","CF4",{"v":0.478,"d":"0.4780"},{"v":0.22,"d":"0.2200"},{"v":0.16,"d":"0.1600"},{"v":7.626,"d":"7.6260"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Heavier than air, light narcotic, Chemical and thermally very stable",{"$nulls":3},68]
[66,"Freon 115","C2CLF5","Freon 14","CF4",{"v":0.521,"d":"0.5210"},{"v":0.24,"d":"0.2400"},{"v":0.164,"d":"0.1640"},{"v":6.892,"d":"6.8920"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","not flammable, narcotic, Chemical & thermal stable, heavier than air.",{"$nulls":3},69]
[67,"Freon C318","C4F6","Freon 14","CF4",{"v":0.369,"d":"0.3690"},{"v":0.17,"d":"0.1700"},{"v":0.185,"d":"0.1850"},{"v":8.397,"d":"8.3970"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},70]
[68,"Germane","GeH4","Ethylene","C2H4",{"v":0.95,"d":"0.9500"},{"v":0.57,"d":"0.5700"},0.1401,{"v":3.418,"d":"3.4180"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},71]
[69,"Germanium Tetrachloride","CECL4","Freon 14","CF4",{"v":0.586,"d":"0.5860"},{"v":0.27,"d":"0.2700"},0.1071,{"v":9.565,"d":"9.5650"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},72]
[70,"Helium","He","Helium","He",{"v":1,"d":"1.0000"},{"v":1.454,"d":"1.4540"},{"v":1.241,"d":"1.2410"},0.1786,{"v":1.04,"d":"1.0400"},5.2014,1.968e-05,5.1931,0.15,null,"Viton","Viton",null,58,null,null,73]
[71,"Hexafluoroethane (Freon 116)","C2F6","Freon 14","CF4",{"v":0.521,"d":"0.5210"},{"v":0.24,"d":"0.2400"},0.1834,{"v":6.157,"d":"6.1570"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},74]
[72,"Hexane","C6H14","Freon 14","CF4",{"v":0.391,"d":"0.3910"},{"v":0.28,"d":"0.2800"},0.3968,{"v":3.845,"d":"3.8450"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},75]
[73,"Hydrogen (n-type)","H2","Hydrogen","H2",{"v":1,"d":"1.0000"},{"v":1.01,"d":"1.0100"},{"v":3.419,"d":"3.4190"},0.0899,{"v":1,"d":"1.0000"},{"v":33.19,"d":"33.1900"},8.92e-06,{"v":14.3,"d":"14.3000"},0.1861,null,"Viton","Viton","Not a linear gas, K-Factor calibration can cause 10% error",44,null,null,76]
[74,"Hydrogen Bromide","HBr ","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.0861,{"v":3.61,"d":"3.6100"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Kalrez","Poison, corrosive, not flammable, heavier than air",{"$nulls":3},77]
[75,"Hydrogen Chloride","HCL ","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.1912,{"v":1.627,"d":"1.6270"},{"v":1,"d":"1.0000"},{"v":324.6,"d":"324.6000"},1.46e-05,0.7987,0.0139,null,"Viton","Kalrez","Poison, bijtend, Corrosive, heavier than air, hydroscopic, if wet only monel & Tantalium",{"$nulls":3},78]
[76,"Hydrogen Cyanide","HCN","Nitrogen probably","N2O/N2",{"v":1.07,"d":"1.0700"},{"v":0.76,"d":"0.7600"},0.3171,{"v":1.206,"d":"1.2060"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton","Very poisonous, flammable, corrosive, with heating polymerisation,explosive with air",null,null,535,79]
[77,"Hydrogen Fluoride","HF","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.3479,{"v":0.893,"d":"0.8930"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Kalrez",null,94,null,null,80]
[78,"Hydrogen Iodide","HI","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.0545,{"v":5.707,"d":"5.7070"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton",{"$nulls":4},81]
[79,"Hydrogen Selenide","H2Se","Nitrogen probably","N2O/N2",{"v":1.112,"d":"1.1120"},{"v":0.79,"d":"0.7900"},{"v":0.10258,"d":"0.1026"},{"v":3.613,"d":"3.6130"},{"v":0.941,"d":"0.9410"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},82]
[80,"Hydrogen Sulfide","H2S","Nitrogen probably","N2O/N2",{"v":1.126,"d":"1.1260"},{"v":0.8,"d":"0.8000"},0.2397,{"v":1.52,"d":"1.5200"},{"v":0.941,"d":"0.9410"},{"v":373.2,"d":"373.2000"},null,{"v":1.004,"d":"1.0040"},0.0143,null,"Viton","Kalrez",null,75,null,null,83]
[81,"Iodine Pentafluoride","IF5","Freon 14","CF4",{"v":0.543,"d":"0.5430"},{"v":0.25,"d":"0.2500"},0.1108,{"v":9.9,"d":"9.9000"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},84]
[82,"Isobutane","CH(CH3)3","Freon 14","CF4",{"v":0.586,"d":"0.5860"},{"v":0.27,"d":"0.2700"},0.3872,{"v":3.593,"d":"3.5930"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},85]
[83,"Isobutylene","C4H6","Freon 14","CF4",{"v":0.63,"d":"0.6300"},{"v":0.29,"d":"0.2900"},0.3701,{"v":2.503,"d":"2.5030"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},86]
[84,"Krypton","Kr","Argon","Ar",{"v":1.002,"d":"1.0020"},{"v":1.453,"d":"1.4530"},0.0593,{"v":3.739,"d":"3.7390"},{"v":1.04,"d":"1.0400"},{"$nulls":5},"Viton","Viton",{"$nulls":4},87]
[85,"Methane","CH4","Nitrogen probably","N2O/N2",{"v":1.014,"d":"1.0140"},{"v":0.72,"d":"0.7200"},0.5328,{"v":0.715,"d":"0.7150"},{"v":0.88,"d":"0.8800"},{"v":190.555,"d":"190.5550"},1.12e-05,{"v":2.232,"d":"2.2320"},0.03389,null,"Viton","Viton",null,75,null,null,88]
[86,"Methanol","CH3OH","Ethylene","C2H4",{"v":0.966,"d":"0.9660"},{"v":0.58,"d":"0.5800"},0.3274,{"v":1.429,"d":"1.4290"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},89]
[87,"Methyl Acetylene","C3H4","Freon 14","CF4",{"v":0.934,"d":"0.9340"},{"v":0.43,"d":"0.4300"},0.3547,{"v":1.787,"d":"1.7870"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},90]
[88,"Methyl Bromide","CH3Br","Ethylene","C2H4",{"v":0.966,"d":"0.9660"},{"v":0.58,"d":"0.5800"},0.1106,{"v":4.236,"d":"4.2360"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","Poison, flammable, heavier than air",null,null,535,91]
[89,"Methyl Chloride","CH3CL","Ethylene","C2H4",{"v":1.05,"d":"1.0500"},{"v":0.63,"d":"0.6300"},0.1926,{"v":2.253,"d":"2.2530"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez","Poison, flammable, explosive mix with air, dangerous with aluminium, zinc & magnesium",{"$nulls":3},92]
[90,"Methyl Fluoride","CH3F","Ethylene","C2H4",{"v":0.957,"d":"0.9570"},{"v":0.68,"d":"0.6800"},{"v":0.322,"d":"0.3220"},{"v":1.518,"d":"1.5180"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},93]
[91,"Methyl Mercaptan","CH3SH","Freon 14","CF4",{"v":1.13,"d":"1.1300"},{"v":0.52,"d":"0.5200"},0.3459,{"v":2.146,"d":"2.1460"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},94]
[92,"Methyl Trichlorosilane","(CH3)SiCL3","Freon 14","CF4",{"v":0.543,"d":"0.5430"},{"v":0.25,"d":"0.2500"},{"v":0.164,"d":"0.1640"},{"v":6.669,"d":"6.6690"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},95]
[93,"Molybdenum Hexafluoride","MOF6","Freon 14","CF4",{"v":0.456,"d":"0.4560"},{"v":0.21,"d":"0.2100"},0.1373,{"v":9.366,"d":"9.3660"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},96]
[94,"Monoethylamine","C2H5NH2","Freon 14","CF4",{"v":0.76,"d":"0.7600"},{"v":0.355,"d":"0.3550"},{"v":0.387,"d":"0.3870"},{"v":2.011,"d":"2.0110"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},97]
[95,"Monomethylamine","CH3NH2","Freon 14","CF4",{"v":0.85,"d":"0.8500"},{"v":0.51,"d":"0.5100"},0.4343,{"v":1.386,"d":"1.3860"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},98]
[96,"Natural Gas","?","Natural Gas","?",{"v":1.014,"d":"1.0140"},{"v":0.72,"d":"0.7200"},0.5328,{"v":0.715,"d":"0.7150"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",null,75,null,null,99]
[97,"Neon","NE","Argon","Ar",{"v":1.006,"d":"1.0060"},{"v":1.46,"d":"1.4600"},{"v":0.246,"d":"0.2460"},{"v":0.9,"d":"0.9000"},{"v":1.04,"d":"1.0400"},{"$nulls":5},"Viton","Viton",{"$nulls":4},100]
[98,"Nitric Oxide","NO","Nitrogen","N2",{"v":0.99,"d":"0.9900"},{"v":0.99,"d":"0.9900"},0.2328,{"v":1.339,"d":"1.3390"},{"v":1,"d":"1.0000"},{"$nulls":5},"Viton","Viton",{"$nulls":4},101]
[99,"Nitrogen","N2","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.2485,{"v":1.25,"d":"1.2500"},{"v":1,"d":"1.0000"},{"v":126.26,"d":"126.2600"},1.79e-05,{"v":1.04,"d":"1.0400"},0.02566,null,"Viton","Viton",null,93,null,null,102]
[100,"Nitrogen Dioxide","NO2","Nitrogen probably","N2O/N2",{"v":1.042,"d":"1.0420"},{"v":0.74,"d":"0.7400"},0.1933,{"v":2.052,"d":"2.0520"},{"v":0.941,"d":"0.9410"},{"v":431,"d":"431.0000"},null,0.8066,0.0132,null,"Viton","Viton",{"$nulls":4},103]
[101,"Nitrogen Trifluoride","NF3","Freon 14","CF4",{"v":1.043,"d":"1.0430"},{"v":0.48,"d":"0.4800"},0.1797,{"v":3.168,"d":"3.1680"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},104]
[102,"Nitrosyl Chloride","NOCL","Ethylene","C2H4",{"v":1.016,"d":"1.0160"},{"v":0.61,"d":"0.6100"},0.1632,{"v":2.92,"d":"2.9200"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},105]
[103,"Nitrous Oxide","N2O","Nitrogen probably","N2O/N2",{"v":1,"d":"1.0000"},{"v":0.71,"d":"0.7100"},0.2088,{"v":1.964,"d":"1.9640"},{"v":0.941,"d":"0.9410"},{"v":309.57,"d":"309.5700"},1.498e-05,0.8795,0.0173,null,"Viton","Viton",{"$nulls":4},106]
[104,"Octafluorocyclobutane (Freon C318)","C4F6","Freon 14","CF4",{"v":0.369,"d":"0.3690"},{"v":0.17,"d":"0.1700"},{"v":0.185,"d":"0.1850"},{"v":8.397,"d":"8.3970"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},107]
[105,"Oxygen","O2","Nitrogen","N2",{"v":1,"d":"1.0000"},{"v":1,"d":"1.0000"},0.2193,{"v":1.427,"d":"1.4270"},{"v":1,"d":"1.0000"},{"v":154.581,"d":"154.5810"},2.05e-05,0.9196,0.02615,null,"Viton","Viton",null,93,null,null,108]
[106,"Oxygen Difluoride","OF2","Ethylene","C2H4",{"v":1.05,"d":"1.0500"},{"v":0.63,"d":"0.6300"},0.1917,{"v":2.406,"d":"2.4060"},{"v":0.941,"d":"0.9410"},{"$nulls":5},"Viton","Viton",{"$nulls":4},109]
[107,"Ozone","O3","Nitrogen","N2",{"v":0.466,"d":"0.4660"},{"v":0.466,"d":"0.4660"},{"v":0.3,"d":"0.3000"},{"v":2.144,"d":"2.1440"},{"v":0.941,"d":"0.9410"},{"$nulls":5},"Viton","Viton",{"$nulls":4},110]
[108,"Pentaborane","B5H9","Freon 14","CF4",{"v":0.565,"d":"0.5650"},{"v":0.26,"d":"0.2600"},{"v":0.38,"d":"0.3800"},{"v":2.816,"d":"2.8160"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},111]
[109,"Pentane","C5H12","Freon 14","CF4",{"v":0.456,"d":"0.4560"},{"v":0.21,"d":"0.2100"},{"v":0.398,"d":"0.3980"},{"v":3.219,"d":"3.2190"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},112]
[110,"Perchloryl Fluoride","CLO3F","Freon 14","CF4",{"v":0.847,"d":"0.8470"},{"v":0.39,"d":"0.3900"},0.1514,{"v":4.571,"d":"4.5710"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},113]
[111,"Perfluoropropane","C3F8","Freon 14","CF4",{"v":0.369,"d":"0.3690"},{"v":0.174,"d":"0.1740"},{"v":0.194,"d":"0.1940"},{"v":8.388,"d":"8.3880"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},114]
[112,"Phosgene","COCL2","Freon 14","CF4",{"v":0.956,"d":"0.9560"},{"v":0.44,"d":"0.4400"},0.1394,{"v":4.418,"d":"4.4180"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},115]
[113,"Phosphine","Ph3","Nitrogen probably","N2O/N2",{"v":1.07,"d":"1.0700"},{"v":0.76,"d":"0.7600"},0.2374,{"v":1.517,"d":"1.5170"},{"v":0.941,"d":"0.9410"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},116]
[114,"Phosphorous Oxychloride","POCL3","Freon 14","CF4",{"v":0.782,"d":"0.7820"},{"v":0.36,"d":"0.3600"},0.1324,{"v":6.843,"d":"6.8430"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},117]
[115,"Phosphorous Pentafluoride","PH5","Freon 14","CF4",{"v":0.652,"d":"0.6520"},{"v":0.3,"d":"0.3000"},{"v":0.161,"d":"0.1610"},{"v":5.62,"d":"5.6200"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},118]
[116,"Phosphorous Trichloride","PCL3","Freon 14","CF4",{"v":0.654,"d":"0.6540"},{"v":0.3,"d":"0.3000"},{"v":0.125,"d":"0.1250"},{"v":6.127,"d":"6.1270"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},119]
[117,"Propane","C3H8","Freon 14","CF4",{"v":0.782,"d":"0.7820"},{"v":0.36,"d":"0.3600"},{"v":0.885,"d":"0.8850"},{"v":1.967,"d":"1.9670"},{"v":0.88,"d":"0.8800"},{"v":369.85,"d":"369.8500"},8.3e-06,{"v":1.696,"d":"1.6960"},0.018,null,"Viton","Viton",null,34,null,null,120]
[118,"Propylene","C3H6","Freon 14","CF4",{"v":0.891,"d":"0.8910"},{"v":0.41,"d":"0.4100"},0.3541,{"v":1.877,"d":"1.8770"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton","flammable, heavier than air, narcotic, with air explosive",39,null,495,121]
[119,"Silane","SiH4","Ethylene","C2H4",{"v":1,"d":"1.0000"},{"v":0.6,"d":"0.6000"},0.3189,{"v":1.433,"d":"1.4330"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},122]
[120,"Silicon Tetrachloride","SiCL4","Freon 14","CF4",{"v":0.608,"d":"0.6080"},{"v":0.28,"d":"0.2800"},{"v":0.127,"d":"0.1270"},{"v":7.58,"d":"7.5800"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},123]
[121,"Silicon Tetrafluoride","SiF4 ","Freon 14","CF4",{"v":0.76,"d":"0.7600"},{"v":0.35,"d":"0.3500"},0.1691,{"v":4.643,"d":"4.6430"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},124]
[122,"Sulfur Dioxide","SO2","Nitrogen probably","N2O/N2",{"v":0.9,"d":"0.9000"},{"v":0.69,"d":"0.6900"},0.1488,{"v":2.858,"d":"2.8580"},{"v":0.941,"d":"0.9410"},{"v":430.7,"d":"430.7000"},1.274e-05,0.6224,0.00994,null,"Viton","Viton",null,65,null,null,125]
[123,"Sulfur Hexafluoride","SF6","Freon 14","CF4",{"v":0.565,"d":"0.5650"},{"v":0.26,"d":"0.2600"},0.1592,{"v":6.516,"d":"6.5160"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},126]
[124,"Sulfuryl Fluoride","SO2F2","Freon 14","CF4",{"v":0.847,"d":"0.8470"},{"v":0.39,"d":"0.3900"},0.1543,{"v":4.562,"d":"4.5620"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},127]
[125,"Tetrafluorahydrazine","N2F4","Freon 14","CF4",{"v":0.695,"d":"0.6950"},{"v":0.32,"d":"0.3200"},{"v":0.182,"d":"0.1820"},{"v":4.64,"d":"4.6400"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},128]
[126,"Trichlorofluoromethane (Freon 11)","CCL3F","Freon 14","CF4",{"v":0.717,"d":"0.7170"},{"v":0.33,"d":"0.3300"},0.1357,{"v":6.129,"d":"6.1290"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},129]
[127,"Trichlorosilane","SiHCL3","Freon 14","CF4",{"v":0.717,"d":"0.7170"},{"v":0.33,"d":"0.3300"},{"v":0.138,"d":"0.1380"},{"v":6.043,"d":"6.0430"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},130]
[128,"1,1,2 Trichloro (Freon 113)","CCL2FCCLF2","Freon 14","CF4",{"v":0.434,"d":"0.4340"},{"v":0.2,"d":"0.2000"},{"v":0.161,"d":"0.1610"},{"v":8.36,"d":"8.3600"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},131]
[129,"Trisobutyl Aluminum","(C4H9)AL","Freon 14","CF4",{"v":0.132,"d":"0.1320"},{"v":0.061,"d":"0.0610"},{"v":0.508,"d":"0.5080"},{"v":8.848,"d":"8.8480"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},132]
[130,"Titanium Tetrachloride","TiCL4","Freon 14","CF4",{"v":0.586,"d":"0.5860"},{"v":0.27,"d":"0.2700"},{"v":0.12,"d":"0.1200"},{"v":8.465,"d":"8.4650"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},133]
[131,"Trichloro Ethylene","C2HCL3","Freon 14","CF4",{"v":0.695,"d":"0.6950"},{"v":0.32,"d":"0.3200"},{"v":0.163,"d":"0.1630"},{"v":5.95,"d":"5.9500"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},134]
[132,"Trimethylamine","(CH3)3N","Freon 14","CF4",{"v":0.608,"d":"0.6080"},{"v":0.28,"d":"0.2800"},{"v":0.371,"d":"0.3710"},{"v":2.639,"d":"2.6390"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},135]
[133,"Tungsten Hexafluoride","WF6","Freon 14","CF4",{"v":0.552,"d":"0.5520"},{"v":0.25,"d":"0.2500"},{"v":0.081,"d":"0.0810"},{"v":13.28,"d":"13.2800"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},136]
[134,"Uranium Hexafluoride","UF6","Freon 14","CF4",{"v":0.434,"d":"0.4340"},{"v":0.2,"d":"0.2000"},0.0888,{"v":15.7,"d":"15.7000"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},137]
[135,"Vinyl Bromide","CH2CHBr","Freon 14","CF4",{"v":1,"d":"1.0000"},{"v":0.46,"d":"0.4600"},0.1241,{"v":4.772,"d":"4.7720"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Viton",{"$nulls":4},138]
[136,"Vinyl Chloride","CH2CHCL","Freon 14","CF4",{"v":1.043,"d":"1.0430"},{"v":0.48,"d":"0.4800"},0.2054,{"v":2.788,"d":"2.7880"},{"v":0.88,"d":"0.8800"},{"$nulls":5},"Viton","Kalrez",{"$nulls":4},139]
[137,"Xenon","Xe","Argon","Ar",{"v":0.993,"d":"0.9930"},{"v":1.44,"d":"1.4400"},0.0378,{"v":5.858,"d":"5.8580"},{"v":1.04,"d":"1.0400"},{"$nulls":5},"Viton","Viton",{"$nulls":4},140]